1. Software description

Welcome to the "Body Composition Measurement and Management System (Bodivista)"

This is the computer-side data management software for the BCA series body composition analyzer developed by Tongfang Health (Beijing) Co., Ltd.,

It can only be connected with the BCA series body composition analyzer produced by our company.

The copyright of this software belongs to Tongfang Health (Beijing) Co., Ltd.

2. Environment and installation

This software is suitable for Windows system computers, including MicroSoft Windows 2007/7/10 series 32-bit and 64-bit environments.

WindowsXP system computers,please use version for windowsXP.

Just copy the folder containing the software to the computer and run the bodivista.exe file in the / bin directory.

You can set it as a desktop shortcut.

Open the home page displayed by bodivista.exe,and then you can see a window like this.

If you use a serial port model, please install the driver of the serial USB adapter cable of the body composition analyzer before use.

The driver is included in this installation package. For 32-bit computer systems, please run dpinst-x86, for 64-bit systems, please run dpinst-amd64 driver installation program.

After installing the driver, plug the serial USB cable into any USB port of the computer and it would be virtualized as a serial port.

3. Connection and settings

The analyzer has two type of product mode with different connection modes: network connection (BCA-1D, BCA-2A) and serial connection (other models).

Please make sure the body composition analyzer has been turned on.

If it is network connection (BCA-1D, BCA-2A) product, connect the network cable to the analyzer from the network port connection, or make sure that the body composition analyzer has been connected to the computer with the serial port USB cable.

The first step in using this software is to set up.Clickto setting.

First, set the Company information. Please enter the Company name and phone number, and click <OK>. This will be displayed on the printed report.

The Company identification code is used for reporting data, which is not required for ordinary users.

Select the network port or serial port connection, and click OK after the selection is complete.

In the network port mode, the network port connection needs to be entered in the network port settings-analyzer IP, enter the analyzer IP address.

When the network cable is connected to the router, the automatically obtained IP address will be displayed on the analyzer screen.

If directly connected to the computer, the IP address is 192.168.0.64.

若与电脑直连,需先配置网络接口ip,推荐配置如图:

则IP地址为192.168.0.64。

At this time, close the connection and settings page, click <Connect> in the upper right corner of the home page, and will connect to the analyzer.

->

The body composition analyzer status will display "Connecting,...", if the instrument is connected normally, it will display "Empty".

* If the connection fails after 10 seconds, please check

(1) Whether the body composition analyzer is turned on normally;

(2) Whether the serial cable (network cable) of the instrument / computer / router is connected well, whether it is loose or stuck. PS: It is recommended to plug and unplug the connection

(3) Find the USB-serial port in the control panel-device manager to see if the COM number matches and the driver is working properly.

If it says "Empty", you can go to test.

Click <Disconnect> next to it to disconnect.

The report sheet style is to choose the report sheet you print. It is divided into “Use professional report paper”, that is, when you print with the report paper we provide, you can use our report paper to print high-definition color reports.

If you only have A4 paper, please choose “Use blank paper”.

The test report mode will fill up all of our printing area and is only used for proofreading the printing position when using professional report paper.

Select the report paper style.

Including BCA-2A / 1A / 1B / 1C / 1D and other basic report paper and water report paper. Please choose according to your instrument model and by your heart.

Click<print mode settings>, you can choose whether to print each of our items, click <Save> to save your settings.

Here, you can choose your working language, support Chinese and English, and take effect when you restart the software.

Here, you can choose the weights and measures you use.SI is the International System and BS is the British system.

4. Personnel information management

For those who regularly test, or those who need unified management, it is necessary to enter into the personnel database in advance, and you can choose it during the test.

Several simulators have been preset in the system for testing. If not needed, it can be deleted.

4.1 Adding and modifying personnel

Modify personnel: Double-click the personnel in the left list, the detailed information can be displayed on the right and can be modified.

After modification, click <Save Person>. When you modify the personnel, all the personnel information in the test data of that id number will be modified together.

Add Person: Please click the <Add Person> button under the [Tester Information] section on the right.

->

Enter the ID, name, gender, year of birth, height, and mobile phone number here. ID can use letters and numbers. Mobile phone number is optional. After filling it out, click <Save Person> to save it in the database and it will appear in the person list on the left.

Delete person: clickto go to Person list

After selecting the person, click <Delete> to delete the person.

4.2 Importing personnel in batches

If you need to enter a large number of person, you can use bulk import.

Use EXCEL / WPS to open the "personnel information import template" file (CSV format), and record according to the personnel information format in the template

After editing, click on the main interface and click <Import person> in the "Person List" to select your csv file to import personnel.

5. Test

The test is divided into real-time acquisition mode and PC control mode. The former is suitable for temporary testing personnel, and the latter is suitable for regular and regular testing personnel, such as members and patients.

5.1 Real-time acquisition mode

After the connection is successful, the tester can directly stand on the body composition analyzer to test, enter the number, gender, height, and age on the instrument touch screen. After the test, the data will automatically appear in the data display area at the bottom of the home page.

In real-time acquisition mode the tester name will auto to “*”.You can change it by mode the person which ID is this.

The main indicators are shown here. For more detailed data and analysis, please check in the report.

During the data collection process, the status of the body composition analyzer above the software will prompt various status information.

5.2 PC control mode

It is strongly recommended that those who regularly test please use the PC control mode to with uniformed the ID and the personal information!

Before starting the PC control test, the body composition analyzer needs to return to the home page. Otherwise, it cannot be controlled!

Double-click to select a person from the left person library, and confirm that the person information appears on the right.

Click <Start PC Control Test> below, the personnel information will be sent to the analyzer, the button on the analyzer screen disappears, and the state of the weight display box is entered.

At this time, the person under test stands on the composition analyzer, holding the handle, the analyzer will automatically start the test. Until the result appears in the data display area of the home page.

[Note] For BCA-1A and BCA-1C component analyzer, after standing on the instrument, please click <Start PC Control Test> again.

After a test is completed, after selecting the next person, you can click <Start PC Control Test> again to start another PC control test.

After all measurements are completed, you can click <Cancel PC Control>, and the buttons on the analyzer screen will be restored.In fact,<Cancel PC Control> automatic exec.

During the PC control process, the status of the body composition analyzer above the software will prompt various status information.

[Note] If the analyzer cannot enter the weight input box screen, please cancel the PC control. After the upper body composition analyzer status displays "Empty", click <Start PC control test> again.

5.3 Batch collection mode

For the test data that is not controlled by the PC, if it needs to be collected into the composition analyzer on a regular basis, the batch collection mode can be used.

After connecting the analyzer, click in home page. Open the batch collection page.

If it is a serial model, you need to enter the query interface on the body composition analyzer and select multiple people to query.

Enter the start and end numbers, once the data entry is found, the software clicks <start> to start collecting once per second, and clicks <end> to end termination the collection early.

If you do not enter the start and end numbers, all data will be transmitted by default.

BCA-1C only supports querying all data.

The network port model analyzer does not need to enter the query interface,just elect the time interval to query the data.

6. Browsing of measurement results

At home page Click. All test data will be displayed here.

<Search> button can be inquired by name.

<Filter> can select specific items, <Graph> button can see the daily change curve of blue items after filtering, if you do not select all the default items

Below <Import Data>, you can import the software in batches and click <Export Data> to export the backup test data to export the test data exported by the old version, or all the data exported by the previous version of the online software.

Click <View Report> to view the selected data report as report paper.

<Print Report> can print out report paper after you are correctly connected to the printer.

There is a brief diagnostic note, indicating your main body composition and possible diseases.

The diagnosis will not appear in the report. If there is no diagnosis result from the imported data of the old version, you can use <Default Diagnosis> to get the judgment made by the body composition software based on the body composition data. If you are a doctor, you can edit the diagnosis result yourself and save it .

The diagnosis result supports the upload of medical records.

<Print Report> can print out the report paper after you connect the printer correctly.

After selecting any number of data, click <Batch Print> to print out all the data you selected. Click <Delete> to delete all the data you selected.

->

On the home page, you can directly select the person, and then click <Check Personnel Data>, all the test records of the person will be automatically searched out.

You can also click on the main interface to browse the current personnel's indicators over time.

7. View report and print report

7.1 View report

The main data area displays the main data. For detailed data, please click <View Report> on the upper right.

->=

You can browse all reports by pulling the scroll bar on the right.

Click <Print> and <Save as PDF> below to print the report and save the PDF file respectively.

7.2 Print report

In addition to the preview print, click the <print> to the right of the view report in the upper right of the main data area to print the report.

7.3 Custom report

If you feel that any kind of report paper can not meet your needs, you can customize the report paper format.

First, you need to design your own report paper style, replace the folder / image / diy-report file (the image size must be 960 * 1358 pixels, JPG format), and then adjust the custom report paper printing parameters, the output can completely match you Demand report. Each item can not be printed ("YES" or "NO"), and the font size and position can also be adjusted.

8. Communication debug

click Change the connect status monitor to manual, you can cancel the default connection and instrument communication connection.

After that, you can click <Manually Query Instrument Status> on the main interface to debug the unknown status

Click to send a test command to the body composition analyzer to test its response and connection validity.

[Note] This function is only for maintenance person.

9. Data export and backup

Click.Then click <Data Export> in the test data list to export all personnel information and measurement results to the specified location (CSV format), which can be opened with EXCEL.

Use the csv format specified in the Document folder to import data into the software.

Click.The entire database file can be backed up to the / backup folder (such as maindb20161010180728.db).

If the main database is damaged, you can rename this file to maindb.db and overwrite the file with the same name in the installation directory / bin folder.

[Note] To ensure data integrity, please back up the database regularly.

Set the backup address to back up the report pictures of each test and enter the backup address to convenience to query.

The import button on the side of the backup data address setting can also import or restore all the data in the old version of the online software by importing the db file in the old version, or the backup db file.

10. Remote connection

10.1 Remote fixed IP server configuration

When you have a cloud platform with a fixed IP address, you can click,

Enter the IP address and port number of your cloud platform as shown in the above picture, so that every data that passes the online software test will be automatically sent to your cloud platform.

The name of the key to upload json can be set in the settings, and the name of the one-key default configuration is to upload data according to the <bodivista http upload protocol>.

In order to prevent manual errors, you need to click <Modify> to edit these items.

After you finish editing, you need to click OK to take effect.

If you do not have a cloud platform, it is recommended to use the Bodivista Cloud Platform address http://47.93.157.150:3001/api/httpResult/.

If you are a confidential organization, please leave this item vacant to protect your data.

10.2 Remote intranet database configuration

If you have a HOSPITAL system remote database, you can complete the connection to the remote database by entering the IP address, database type, database name and database user name password of your remote database.

If you don't have a remote database, please select "Not connect".

The software supports SQLServer, MySQL, MySQL-ODBC database connection methods, pay attention to the case and input method when filling in the database user name password.

In order to prevent mistakes, you need to click <Modify> to edit these items. After editing, you need to click <Save> to take effect.

After the configuration is completed, click <Remote Database Staffing> You need to configure the names of the personnel information and measurement result information tables in the remote database and the names of the items. Red is required, personnel information on the left, and measurement results on the right.

If your remote database does not have this item, please let it blank.

If you have configured the personnel list, you can search for the personnel in the remote database by name or number on the main interface.

->

If you have configured all project information, you can click on the main interface to upload the data you selected to the remote server.

In the configuration interface

When selecting “Automatic connection-upload”, the system will automatically upload to the remote server after the test is completed.

If it is filled out”Not auto uploaded ”, the system will upload your test data only if you click.

10.3 ftp server configuration

When the ftp service is enabled on your server, you can configure the ftp server IP, interface, user name, and password to enable the software to connect to your ftp server.

This software uploads the report paper containing the measurement results to the specified path of the ftp server you set in the format of jpg.

ftp service default port number is 21

Similarly, when you select automatic connection-automatic upload, the system will automatically upload to the remote server after the test is completed.

If it is filled out”Not auto uploaded ”, the system will upload your test data only if you click.

If you do not have an ftp server, please choose “Not to connect”.

bodytype | bodytype
1 | Invisible Fat
2 | Lightly Muscled
3 | Thin
4 | Fatty
5 | Fit
6 | Low Fat
7 | Obese
8 | Muscular
9 | Athletic